TRUE

TRUE

FALSE

FALSE

FALSE

TRUE

TRUE

FALSE

Reset upon opening COM port connection

Send ID packet to computer

Check if rx byte is 0x00

Check retry counter

Flash panel LED 3x

Parse setup packet and load values

Load default setup values

Check if setup packet and values are valid

Reset retry counter

Clear rx serial buffer and set retry counter

Retrieve next byte in rx serial buffer

Retrieve all data in the rx serial buffer

Check if default setup values are valid

Repeat setup packet back to computer

Apply setup and start driver run loop

Decrement retry counter